//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
//BASE_SET   tsinghua set 01 ambe set +2c 03 st24set 06 ambe 3000 set 00 
.Set VOCODER_VAR = 03
.Set MODGAIN_VAR = 08
.Set ID_VAR = 01
.Set CC_VAR = 01
.Set FRAME_VAR = 00
.Set SILENCE_VAR = 00


//Call match test, 
//.Set ID_VAR = 05

//Voice call with 19 02, and Mod_Gain inverted
//.Set MODGAIN_VAR = F8

//Call match test, CC code not matched
//.Set CC_VAR = 02

//Voice call with extended header
//.Set FRAME_VAR = 03

//Voice call with extended preamble and silence
//.Set SILENCE_VAR = 27



Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 {VOCODER_VAR}
Receive	Command:84 A9 61 00 02 00 10 00
Pause 3000
Command ID:	Set Digital Mod gain
Send	Command: 84 A9 61 00 03 00 2C {MODGAIN_VAR} 00
 Receive	Data:84 A9 61 00 02 00 2C 00
Command ID:	DMR_CC
Send	Command: 84 A9 61 00 02 05 77 {CC_VAR}
Receive	Data:84 A9 61 00 02 05 77 00
Command ID:	DMR_CALL_OPTION 
Send	Command: 84 A9 61 00 06 05 79 81 {SILENCE_VAR} {FRAME_VAR} 00  00 
Receive	Data:84 A9 61 00 02 05 79 00
Pause 1000

Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 02 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 02
Receive	Data:84 A9 61 00 02 00 1A 00


Command ID:	DPMR_DATA_FRAME
Send	Command: 84 A9 61 00 0c 05 43 01 09 00 00 00 FF FF FF 00 00 01
Receive	Command:84 A9 61 00 01 20 43 
Command ID:	DPMR_DATA_FRAME
Send	Command: 84 A9 61 00 0c 05 43 11 09 00 00 00 FF FF FF 00 00 01
Receive	Command:84 A9 61 00 01 20 43 

