//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

.Set READY_VAR = 01

Command ID:	VOCODER_CMODE
Send	Command: 84 A9 61 00 02 00 02 0A
Receive	Data:84 A9 61 00 02 00 02 00

Command ID:	DPMR_CC
Send	Command: 84 A9 61 00 04 03 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 03 5C 00
Command ID: WORK_MODE_DUPLEX
Send command: 84 A9 61 00 04 00 18 03 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 03
//Send command: 84 A9 61 00 02 00 1A 04
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	ADDRESSING_MODE
Send	Command: 84 A9 61 00 02 03 28 01
Receive	Command:84 A9 61 00 02 03 28 00
Command ID: DPMR_HT_CI
Send command: 84 A9 61 00 03 03 57 00 00
Receive Data: 84 A9 61 00 02 03 57 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 12 34 56 70
Receive Data: 84 A9 61 00 02 03 52 00
Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 12 34 56 70
Receive Data: 84 A9 61 00 02 03 53 00
Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D ff
Receive	Command:84 A9 61 00 02 00 1D 00
Command ID:	DEMOD_GAIN
Send	Command: 84 A9 61 00 03 00 1C 00 00
Receive	Command:84 A9 61 00 02 00 1C 00
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 1a
Receive	Command:84 A9 61 00 02 00 20 00
//Receive	Data:84 A9 61 00 02 30 1B 09
Receive	Data:84 A9 61 00 02 30 1B 04
Receive Data: 84 A9 61 00 03 30 57 00 00
Receive Data: 84 A9 61 00 02 30 54 1a
Receive Data: 84 A9 61 00 04 30 50 1B 91 FD
Receive Data: 84 A9 61 00 04 30 51 1B 91 FD
Receive	Command:84 A9 61 00 05 30 52 12 34 56 70
Receive	Command:84 A9 61 00 05 30 53 12 34 56 70
Receive	Command:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 30 27 00
Pause 500

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 80 F3
Receive	Data:84 A9 61 00 04 30 08 03 80 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 81 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 81 F3
Receive	Data:84 A9 61 00 04 30 08 03 81 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 81 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 82 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 82 F3
Receive	Data:84 A9 61 00 04 30 08 03 82 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 82 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 83 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 83 F3
Receive	Data:84 A9 61 00 04 30 08 03 83 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 83 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 84 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 84 F3
Receive	Data:84 A9 61 00 04 30 08 03 84 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 84 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 85 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 85 F3
Receive	Data:84 A9 61 00 04 30 08 03 85 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 85 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 86 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 86 F3
Receive	Data:84 A9 61 00 04 30 08 03 86 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 86 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 87 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 87 F3
Receive	Data:84 A9 61 00 04 30 08 03 87 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 87 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 88 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 88 F3
Receive	Data:84 A9 61 00 04 30 08 03 88 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 88 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 89 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 89 F3
Receive	Data:84 A9 61 00 04 30 08 03 89 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 89 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8A F3
Receive	Data:84 A9 61 00 04 30 08 03 8A F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8B F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8B F3
Receive	Data:84 A9 61 00 04 30 08 03 8B F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8B F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8C F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8C F3
Receive	Data:84 A9 61 00 04 30 08 03 8C F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8C F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8D F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8D F3
Receive	Data:84 A9 61 00 04 30 08 03 8D F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8D F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8E F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8E F3
Receive	Data:84 A9 61 00 04 30 08 03 8E F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8E F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8F F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8F F3
Receive	Data:84 A9 61 00 04 30 08 03 8F F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8F F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100




Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 20 F3
Receive	Data:84 A9 61 00 04 30 08 03 20 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 05 F3
Receive	Data:84 A9 61 00 04 30 08 03 05 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 0A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 0A F3
Receive	Data:84 A9 61 00 04 30 08 03 0A F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 0A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 10 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 10 F3
Receive	Data:84 A9 61 00 04 30 08 03 10 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 10 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 20 F3
Receive	Data:84 A9 61 00 04 30 08 03 20 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 30 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 30 F3
Receive	Data:84 A9 61 00 04 30 08 03 30 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 30 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 40 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 40 F3
Receive	Data:84 A9 61 00 04 30 08 03 40 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 40 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 50 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 50 F3
Receive	Data:84 A9 61 00 04 30 08 03 50 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 50 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 60 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 60 F3
Receive	Data:84 A9 61 00 04 30 08 03 60 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 60 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 70 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 70 F3
Receive	Data:84 A9 61 00 04 30 08 03 70 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 70 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 7A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 7A F3
Receive	Data:84 A9 61 00 04 30 08 03 7A F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 80 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 80 D0
Receive	Data:84 A9 61 00 04 30 08 03 80 CE
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 20 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 20 D0
Receive	Data:84 A9 61 00 04 30 08 03 20 CF
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 05 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 05 D0
Receive	Data:84 A9 61 00 04 30 08 03 05 CF
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 7A D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 7A D0
Receive	Data:84 A9 61 00 04 30 08 03 7A CF
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7A D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Pause 4000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 80 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 20 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 05 F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 7a F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 7A F3
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7a F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 80 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 80 D0
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 20 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 20 D0
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 05 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 05 D0
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 7a D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 7A D0
Pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7a D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
Pause 100



Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00 
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	Command:84 A9 61 00 04 30 4B 00 00 00
Pause 1000
Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Command:84 A9 61 00 02 00 18 00
