//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

Command ID:	CHIP_RESET
Send	Command: 84 A9 61 00 01 00 14 00
Receive	Data:84 A9 61 00 02 20 17 01
PAUSE 2000
Command ID:	ACTIVATION
Send	Command: 84 A9 61 00 31 00 38 53 43 54 33 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 08 00 00 00 00 28 cc 66 2c 4b 9f 01 24 3b fc ed 92 10 b6 6f dc 00
//Receive	Data:84 A9 61 00 03 00 39 2F 15
Receive	Data:84 A9 61 00 02 00 38 00
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 00
Receive	Data:84 A9 61 00 02 00 10 00
Receive	Data:84 A9 61 00 03 00 39 2F 15
pause 4000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 20
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 1000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 00
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 2000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 30
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 1000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 00
PAUSE 2500
Receive Data: 84 A9 61 00 02 00 15 00
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 33
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 1000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 00
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 2000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 34
PAUSE 1000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 00
Receive Data: 84 A9 61 00 02 00 15 00
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 1000
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 35
PAUSE 100
Button INT0
PAUSE 1000
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
PAUSE 1000
//Command ID:	LOW_POWER
//Send	Command: 84 A9 61 00 02 00 15 36
//Button NIMI 2000
//PAUSE 2000
//Receive	Command:84 A9 61 00 02 20 17 01
//Receive	Command:84 A9 61 00 03 00 39 2F 15
//PAUSE 1000
Command ID:	ACTIVATION
Send	Command: 84 A9 61 00 31 00 38 53 43 54 33 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 08 00 00 00 00 28 cc 66 2c 4b 9f 01 24 3b fc ed 92 10 b6 6f dc 00
//Receive	Data:84 A9 61 00 03 00 39 2F 15
Receive	Data:84 A9 61 00 02 00 38 00
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 00
Receive	Data:84 A9 61 00 02 00 10 00
Receive	Data:84 A9 61 00 03 00 39 2F 15
pause 2000
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 03
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 1000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 00
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 2000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 04
PAUSE 1000
Command ID: LOW_POWER
Send command: 84 A9 61 00 02 00 15 00
Receive Data: 84 A9 61 00 02 00 15 00
Receive Data: 84 A9 61 00 02 00 15 00
PAUSE 1000
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 05
PAUSE 100
Button INT0
PAUSE 1000
Receive	Command:84 A9 61 00 02 00 15 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00
PAUSE 1000
//Command ID:	LOW_POWER
///Send	Command: 84 A9 61 00 02 00 15 06
//Button NIMI 2000
//Receive	Command:84 A9 61 00 02 20 17 01
//Receive	Command:84 A9 61 00 03 00 39 2F 15
//PAUSE 1000
Command ID:	ACTIVATION
Send	Command: 84 A9 61 00 31 00 38 53 43 54 33 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 08 00 00 00 00 28 cc 66 2c 4b 9f 01 24 3b fc ed 92 10 b6 6f dc 00
Receive	Data:84 A9 61 00 02 00 38 00
Command ID:	LOW_POWER
Send	Command: 84 A9 61 00 02 00 15 00
Receive	Command:84 A9 61 00 02 00 15 00


