//Verison=2.0
//Example,Don't Delete flowing text, 涓嬮潰鏄緥瀛?璇蜂笉瑕佸垹闄?
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary:缁撴潫閫氳瘽 // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '61 00 02 00 19 00' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 03
Receive	Command:84 A9 61 00 02 00 10 00
Command ID:	DPMR_CC
Send	Command: 84 A9 61 00 04 03 5C 7D F5 DF
Receive	Command:84 A9 61 00 02 03 5C 00
Command ID: WORK_MODE_DUPLEX
Send command: 84 A9 61 00 04 00 18 02 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 03
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	ADDRESSING_MODE
Send	Command: 84 A9 61 00 02 03 28 01
Receive	Command:84 A9 61 00 02 03 28 00
//Command ID: DPMR_CI
//Send command: 84 A9 61 00 03 03 5A 24 00
//Receive Data: 84 A9 61 00 02 03 5A 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 12 34 56
Receive Data: 84 A9 61 00 02 03 50 00
Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 04 03 51 12 34 56
Receive Data: 84 A9 61 00 02 03 51 00
Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D 7f
Receive	Command:84 A9 61 00 02 00 1D 00
//VOICE APPENDED
Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 A2    
Receive	Command:84 A9 61 00 02 00 20 00
//data 2
//Command ID:	CALL_START
//Send	Command: 84 A9 61 00 02 00 20 62    
//Receive	Command:84 A9 61 00 02 00 20 00